1-100 packets transmitted, 99 received, 1% packet loss, time 10117ms

rtt min/avg/max/mdev = 23.912/93.384/377.679/65.942 ms, pipe 4

2-100 packets transmitted, 38 received, +21 errors, 62% packet loss, time 33389ms

rtt min/avg/max/mdev = 1119.969/11849.353/28504.088/10475.544 ms, pipe 67

3-100 packets transmitted, 59 received, 41% packet loss, time 10568ms

rtt min/avg/max/mdev = 499.968/3540.493/6332.685/1899.529 ms, pipe 59

4-100 packets transmitted, 32 received, 68% packet loss, time 10739ms

rtt min/avg/max/mdev = 619.639/5127.014/9855.844/3916.361 ms, pipe 68

5-100 packets transmitted, 78 received, 22% packet loss, time 10565ms

rtt min/avg/max/mdev = 29.977/1043.241/3254.242/1023.924 ms, pipe 31

6-100 packets transmitted, 52 received, +6 errors, 48% packet loss, time 19123ms

rtt min/avg/max/mdev = 1496.328/4686.252/9704.670/2382.518 ms, pipe 36

7-100 packets transmitted, 38 received, +21 errors, 62% packet loss, time 33389ms

rtt min/avg/max/mdev = 1119.969/11849.353/28504.088/10475.544 ms, pipe 67

pi@raspberrypi:~ $ sudo ping -c 100 -s 8192 -i .1 10.208.5.34

8-100 packets transmitted, 97 received, 3% packet loss, time 10218ms

rtt min/avg/max/mdev = 21.462/95.151/340.060/68.114 ms, pipe 4

9-100 packets transmitted, 99 received, 1% packet loss, time 10212ms

rtt min/avg/max/mdev = 22.590/110.902/347.429/70.739 ms, pipe 4

10-100 packets transmitted, 88 received, 12% packet loss, time 10402ms

rtt min/avg/max/mdev = 30.121/405.159/1769.896/411.868 ms, pipe 17

Obs: errors é igual destinantion host unreachable