1-100 packets transmitted, 99 received, 1% packet loss, time 99518ms

rtt min/avg/max/mdev = 14.209/355.150/2520.286/447.717 ms, pipe 3

2-100 packets transmitted, 53 received, 47% packet loss, time 101388ms

rtt min/avg/max/mdev = 27.150/877.281/3620.617/893.168 ms, pipe 4

3-100 packets transmitted, 94 received, 6% packet loss, time 99506ms

rtt min/avg/max/mdev = 14.665/251.692/2312.635/370.548 ms, pipe 3

4-100 packets transmitted, 35 received, +15 errors, 65% packet loss, time 101868ms

rtt min/avg/max/mdev = 97.449/1866.486/12482.901/3141.390 ms, pipe 9

5-100 packets transmitted, 100 received, 0% packet loss, time 99191ms

rtt min/avg/max/mdev = 14.642/210.710/1746.051/232.445 ms, pipe 2

6- 100 packets transmitted, 94 received, 6% packet loss, time 99886ms

rtt min/avg/max/mdev = 29.232/522.757/3012.518/475.877 ms, pipe 3

7-100 packets transmitted, 96 received, 4% packet loss, time 99567ms

rtt min/avg/max/mdev = 25.706/448.955/1969.968/430.074 ms, pipe 2

8-100 packets transmitted, 100 received, 0% packet loss, time 99208ms

rtt min/avg/max/mdev = 15.679/273.956/1518.980/244.783 ms, pipe 2

9-100 packets transmitted, 98 received, 2% packet loss, time 99583ms

rtt min/avg/max/mdev = 25.261/451.299/1765.221/374.077 ms, pipe 2

10-100 packets transmitted, 99 received, 1% packet loss, time 99273ms

rtt min/avg/max/mdev = 14.620/261.392/1719.723/274.483 ms, pipe 2